Per Formula SAE Rule T12.1.3, the following transponder types are approved for the Formula SAE 2017 events in Michigan and Lincoln:

* AMB / MyLaps TranX260 transponders (red color)
* MYLAPS X2 Car/Bike transponders

If you own a functional AMB MyLaps TranX260 it does not need to be replaced.

The MX (orange color) or X2 MX transponders used by the Baja SAE events will not work with the Formula SAE timing system.